Contractor Letter Head

Method of Statement for Temporary Connection of Drainage Pipe to TAQA Water Solutions Manhole
	Sector : 
	

	Plot     :
	

	Owner Name :
Consultant     :
	

	Contractor     :
	


1.Scope 

The scope covers the procedure for temporary connections of drainage pipe to TAQA Water Solutions manhole.

2.Purpose

To define the method and criteria for connection, operation, maintenance and responsibility to ensure no odor and no damage to TAQA Water Solutions Asset.

3.Connection Procedures 

General Requirements

· Ensure all safety requirements and its compliance.

· Temporary fencing should be approved prior to temporary connection works.
· TAQA Water Solutions manhole should be outside temporary fence.

· Temporary manholes for Temporary Utilities should be inside the plot limits.
· TAQA Water Solutions Approved “Temporary Connection Drawings & Method Statements of Connections” are in the workplace for connection reference.

· Examine surfaces in preparation to installation of drainage pipes for   compliance.
· General requirements for piping systems should comply with the TAQA Water Solutions.

Connections to TAQA Water Solutions Manholes
· Investigate areas & its condition prior to installations.

· Install piping systems according to Approved Temporary Connection drawings & method statement procedures.

· Connect to TAQA Water Solutions manholes specified for the plot under supervision of TAQA Water Solutions Inspector.

· Connections should comply with the standard procedures of permanent connections to ensure no odor to escape & no damage to TAQA Water Solutions properties.

· All piping materials should be handled according to manufacturer’s instructions.
4.Operations

· Cover the manholes after inspection and approval prior to operation.

· Apply identifying markers & flow directions to pipe works for ready references.

· Locate signs as maybe required.

Maintenance 

· Clean interior of piping system. Remove dirt and debris as work progress.

· Protect drainage pipes during construction period to avoid clogging and accidental damages to surrounding forces.

Responsibility 

· It is the full responsibility of the contractor to comply with the “ Letter of Undertaking” provided to ensure that the area utilized for temporary connection purposes are maintained, no damages , clean and free of debris.
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